[DEVICE]
Name=P12F675
Clock=4000000
[MEMORY_MODEL]
Value=0
[BUILD_TYPE]
Value=0
[ACTIVE_TAB]
Value=ShockSensor.c
[USE_EEPROM]
Value=0
[USE_HEAP]
Value=0
[HEAP_SIZE]
Value=2000
[EEPROM_DEFINITION]
Value=
[FILES]
Count=1
File0=ShockSensor.c
[BINARIES]
Count=0
[IMAGES]
Count=0
ActiveImageIndex=-1
[OPENED_FILES]
Count=1
File0=ShockSensor.c
[EEPROM]
Count=0
[ACTIVE_COMMENTS_FILES]
Count=0
[OTHER_FILES]
Count=0
[SEARCH_PATH]
Count=3
Path0=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\Defs\
Path1=C:\Users\Public\Documents\Mikroelektronika\mikroC PRO for PIC\Uses\P16\
Path2=C:\Users\karolysi\Desktop\Shock_sensor\FW\
[HEADER_PATH]
Count=0
[HEADERS]
Count=0
[PLDS]
Count=0
[Useses]
Count=22
File0=ADC
File1=Button
File2=Conversions
File3=C_Math
File4=C_Stdlib
File5=C_String
File6=C_Type
File7=EEPROM
File8=Lcd
File9=Lcd_Constants
File10=Manchester
File11=MemManager
File12=One_Wire
File13=PS2
File14=Software_I2C
File15=Software_SPI
File16=Software_UART
File17=Sound
File18=Sprinti
File19=Sprintl
File20=Time
File21=Trigonometry
[EXPANDED_NODES]
Node0=Sources
Count=1
